Fixed Price Schedule

**CONTRACT PRICE BREAKDOWN**

(To Be Completed By The PROPONENT)

All prices (in Bermuda dollars) are to be all inclusive of all other associated works as shown on the Contract Documents, including materials, related accessories, storage, transport, assembly, placement, coordination w/ MPW, and overhead and profit. These rates may be used for determining additions and deletions from the contract sum and for interim payment valuation.

|  |  |  |
| --- | --- | --- |
| **ITEM** | **DESCRIPTION** |  **LUMP SUM** |
|  | Mobilization & temporary facilities |  |
|  | Traffic control |  |
|  | Demolition and Disposal |  |
|  | Deck Reinstatement |  |
|  | Curb and sidewalk Reinstatement |  |
|  | Handrail Reinstatement |  |
|  | Demobilization |  |
|  |  |  |
|  | **TOTAL**  |  |

**NOTE:** All work detailed on the Contract Documents shall be covered completely by the Total Lump Sum. Individual lump sum items are all-inclusive. If a specific task is not identified separately in the above list, the Contractor shall assume that it is included as part of another related listed item or items, and shall base his lump sum amounts on this assumption. The price shall include, indicate separately, the cost of any work permits, and taxes.

UNIT RATE SCHEDULE

(To Be Completed By The Contractor)

All prices (in Bermuda dollars) in the schedule are to be **inclusive of materials, tools and related accessories, storage, transport, plant and equipment (staging, platforms etc. to work on deck edge) assembly, placement, access, wastage, coordination with MPW and overhead and profit.** These rates may be used for determining additions to, and deletions from, the contract sum.

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **Unit**  | **Rate** |
|  | Site Supervisor | Hr |  |
|  | Skilled Labour - concreting | hr |  |
|  | Skilled Labour - welding | hr |  |
|  | Skilled Labour - other | hr |  |
|  | Unskilled Labour | hr |  |
|  | Manned Traffic Control (stop-go lollipops, pair) | hr |  |
|  | Supply and install 12mm galvanized steel rebar | LF |  |
|  | Supply and install 16mm galvanized steel rebar | LF |  |
|  | Supply and install concrete grade 25MPa (3600psi) | yd3 |  |
|  | Additional troughing patch repair | sqft |  |
|  | Equipment/ truck | day |  |
|  | Equipment/ crane | day |  |
|  | Equipment/ excavator | day |  |
|  | Equipment/ Boat & Barge | day |  |
|  | **Other items not listed above** |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

For variations to the contract not covered in the preceding price breakdown rates or the above schedule of unit rates, the price may be determined on the basis of the base material and installation cost plus \_\_\_\_\_% for overhead and \_\_\_\_\_% for profit and applied separately to the base cost.

**Note: Amendment/addenda will be posted at** [**https://www.gov.bm/procurement-notices**](https://www.gov.bm/procurement-notices)**. Respondents should visit the Government Portal website on a regular basis during the Procurement process.**